{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["MainPage","Initial","Transport Input Data","Test","EnergyPerformanceData","LocalEnergySupplyData","Lists","KPIResults","KPIs summary list"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":82,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MainPage","index":0,"n_rows":28,"n_cols":9,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["PI-SEC Scenario Calculator","Front Page"]
["Neighbourhood:","Furuset"]
[]
["Climate Zone","1. Sør-Norge, innland"]
[]
["KEY DATA","Now","End of project"]
["Project timeframe",2015,2030]
["Area"]
["Population",280]
["Number of jobs",150]
["Area of buildings (m2 BRA)",25000]
["Number of buildings",2]
[]
["GOALS","KPI","Category","Sub category","Sector","Unit","Comparison","Relative to","Goal at EoP"]
[]
[]
[]
[]
["Menu"]
[]
[]
[]
[]
[]
[]
[]
["Scenarioes"]
["Initial"]

{"sheet":"Initial","index":1,"n_rows":66,"n_cols":50,"rows_kept":66,"cut":false,"hidden":false,"merged":[[3,7,3,12],[4,13,4,21],[3,14,3,39],[4,23,4,30],[4,32,4,39],[44,4,44,8],[43,4,43,9],[12,10,12,35],[12,36,12,43],[4,43,4,46]]}
[{"$f":"MainPage!A1","v":"PI-SEC Scenario Calculator"},"Initial Situation",{"$f":"ProjectStart","v":2015}]
["Neighbourhood",{"$f":"MainPage!B2","v":"Furuset"}]
["Buildings"]
["General description",null,null,null,null,null,null,"Energy performance",null,null,null,null,null,null,"Thermal Energy supply system",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Renewable energy production",null,null,null,null,null,null,"Emission Data","Construction site data"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Heating",null,null,null,null,null,null,null,null,null,"Hot Water",null,null,null,null,null,null,null,null,"Cooling",null,null,null,null,null,null,null,"Solar Thermal (surplus)",null,null,"Solar PV (total)",null,null,null,"Materials","Construction Machines","Thermal energy"]
["Building","Category","Year of construction","Area [m2]","Ownership","residents/ employees\n[#]","Res above 13y/ Other Users \n[#]","Energy certificate","Performance\ninput","Heating \n[kWh/m2]","Hot Water\n[kWh/m2]","Cooling\n[kWh/m2]","Electricity\n[kWh/m2]","Source 1","Coverage \n[%]","Efficiency/COP\n[-]","Source 2","Coverage \n[%]","Efficiency/COP\n[-]","Source 3","Coverage \n[%]","Efficiency/COP\n[-]","Source 1","Coverage \n[%]","Efficiency/COP\n[%]","Source 2","Coverage \n[%]","Efficiency/COP\n[%]","Source 3","Coverage \n[%]","Efficiency/COP\n[%]","Source 1","Coverage \n[%]","Efficiency/COP\n[-]","Source 2","Coverage \n[%]","Efficiency/COP\n[%]","Source 3","Coverage \n[%]","Efficiency/COP\n[%]","Size\n[m2]","Peak production\n[kWp]","Yearly production \n[kWh]","Size\n[m2]","Input \ntype","Peak production\n[kWp]","Yearly production \n[kWh]","Life cycle emission\n[tCO2 eqv./y]","Fuel","Fuel"]
["Building 1","Residential apartment building",1988,20000,"Housing cooperative",280,25,"F","TEK 87",99.7,29.8,0,35.1,"Electric heater",1,0.88209000000000004,null,null,null,null,null,null,"Electric water heater",1,0.58211999999999997]
["Building2","Office building",2000,5000,"Private",150,105,"E","TEK 97",78.3,5,20.8,100.30000000000001,"Heat pump",0.7,2.2529249999999998,"Electric boiler",0.3,0.85651999999999995,null,null,null,"Heat Pump",0.6,1.4228999999999998,"Electric bolier",0.4,0.54,null,null,null,"Local Chiller",1,2.4500000000000002]
[]
[null,null,null,null,null,null,null,null,null,0,0,0,0]
[]
["Infrastructure"]
["General description",null,null,"Energy performance"]
["Outdoor lighting","Year of installation","# units","Energy performance\nCategory","Energy consumption\n[kWh/unit]"]
["Street1",2010,200,"High efficicency",160]
[]
["Snow Melt Systems","Year of installation","Size [m2]","Energy performance\nCategory","Energy consumption\n[kW/m2]","Energy source","Efficiency/COP\n[-]"]
["Street1",2010,400,"High efficicency",100,"Electric boiler",0.85651999999999995]
[]
[]
["Local energy plant"]
["Energy Source",null,null,null,"Heating to District Heating system",null,"Cooling to District Cooling system",null,"Electricity to grid"]
["Type","Energy Source","CO2 Emission\n[g/kWh]","Efficiceny\n[%]","Capacity\n[kW]","Production\n[kWh]","Capacity\n[kW]","Production\n[kWh]","Capacity\n[kW]","Production\n[kWh]"]
[]
[]
[]
["District Heating"]
["Energy Source",null,null,null,"Distribution"]
["Heat Source","Coverage [%]","CO2 Emission\n[g/kWh]","Production \nefficiency\n[%]","Distribution\n losses"]
["Electricity",0.28199999999999997,123,0.95,0.1]
["Heat Pump",7.9000000000000001E-2,123,3.125]
["Solar Collector",null,0,1]
["Waste Heat",null,0,0.9]
["Waste Incineration",0.57599999999999996,11,0.9]
["Wood Chips",null,18,0.9]
["Pellets",{"$f":"5.3%*32.8%","v":1.7383999999999997E-2},19,0.9]
["Bio-oil",{"$f":"5.3%*67.2%","v":3.5616000000000002E-2},10,0.9]
["Bio-gas",null,10,0.9]
["Fossile Oil",2E-3,268,0.9]
["LPG",8.0000000000000002E-3,235,0.9]
[]
[]
["Transport"]
["Population",null,null,null,"Trip Generation",null,null,null,null,null,"Travel method distribution",null,null,null,null,null,"Location:",null,"Oslo, Groruddalen",null,null,null,"Other Travel Data",null,null,null,null,null,"Parking Capacity"]
[null,null,null,null,"Users",null,null,null,null,"Other Users","Work",null,null,"Service",null,null,"Private errand",null,null,"Other",null,null,"Average distance",null,"# passengers",null,null,"Public Transport","Factor","Distribution of reduction"]
["Building Category","Area [m2]","residents/ employees\n[#]","Res above 13y/ Other Users \n[#]","Work","Service","Private errand","Utside Service","Goods transport",null,"Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Public\nTransport","Car","Buss","Rail","Car","% using track","1-0","Walk/\nBike","Public\nTransport","Car sharing"]
["Residential individual housing",{"$f":"SUMIF(BuildingCategoryRange,A47,BuildingAreaRange)","v":0},{"$f":"SUMIF(BuildingCategoryRange,A47,BuildingResidentsRange)","v":0},{"$f":"SUMIF(BuildingCategoryRange,A47,BuildingUserRange)","v":0},0.8,0.1,1,1.7,0.1,0,0.11,0.5,0.39,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,{"$f":"NA()","v":{"$error":"#N/A"}},{"$f":"NA()","v":{"$error":"#N/A"}},{"$f":"NA()","v":{"$error":"#N/A"}},{"$f":"NA()","v":{"$error":"#N/A"}}]
["Residential apartment building",20000,280,25,0.8,0.1,1,1.7,0.1,0,0.11,0.5,0.39,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,{"$f":"NA()","v":{"$error":"#N/A"}},{"$f":"NA()","v":{"$error":"#N/A"}},{"$f":"NA()","v":{"$error":"#N/A"}},{"$f":"NA()","v":{"$error":"#N/A"}}]
["Office building",5000,150,105,1.6,0.6,0.2,0.1,0.2,1.43,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["Kindergarten",0,0,0,1.6,0.6,0.2,0.1,0.2,0.79,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["School",0,0,0,1.6,0.6,0.2,0.1,0.2,0.83,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["University/Collage",0,0,0,1.6,0.6,0.2,0.1,0.2,0.83,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["Hospital",0,0,0,1.6,0.6,0.2,0.1,0.2,2,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["Nursing home",0,0,0,1.6,0.6,0.2,0.1,0.2,2,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["Hotel",0,0,0,1.6,0.6,0.2,0.1,0.2,2.4500000000000002,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["Sports Facility",0,0,0,1.6,0.6,0.2,0.1,0.2,0,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["Comercial building",0,0,0,1.6,0.2,0.1,0.1,1,1.65,0.11,0.5,0.39,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["Cultural building",0,0,0,1.6,0.6,0.2,0.1,0.2,1.65,0.11,0.5,0.39,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
["Industry/Workshop",0,0,0,1.6,0.2,0.1,0.1,1,0,0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,13.8,16,19.399999999999999,100,1.3,0.6,1,0.15,0.75,0.1]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"}]
["CO2 emission factors"]
["Means of transport","Fossile \n[g/km]","NonFossile \n[g/km]","% NonFossile"]
["Buss",780,230,0]
["Rail",0,3900,1]
["Car",140,45,8.1000000000000003E-2]
["Truck",440,85,1.7000000000000001E-2]

{"sheet":"Transport Input Data","index":2,"n_rows":111,"n_cols":21,"rows_kept":111,"cut":false,"hidden":true,"merged":[[2,1,2,6],[3,1,3,5]]}
["Transport Data"]
[]
["BuildingCategory","Trip Generation"]
[null,"Users",null,null,null,null,"Other Users"]
[null,"Work","Service","Private errand","Utside Service","Goods transport"]
["Residential individual housing",0.8,0.1,1,1.7,0.1,0]
["Residential apartment building",0.8,0.1,1,1.7,0.1,0]
["Office building",1.6,0.6,0.2,0.1,0.2,1.43]
["Kindergarten",1.6,0.6,0.2,0.1,0.2,0.79]
["School",1.6,0.6,0.2,0.1,0.2,0.83]
["University/Collage",1.6,0.6,0.2,0.1,0.2,0.83]
["Hospital",1.6,0.6,0.2,0.1,0.2,2]
["Nursing home",1.6,0.6,0.2,0.1,0.2,2]
["Hotel",1.6,0.6,0.2,0.1,0.2,2.4500000000000002]
["Sports Facility",1.6,0.6,0.2,0.1,0.2,0]
["Comercial building",1.6,0.2,0.1,0.1,1,1.65]
["Cultural building",1.6,0.6,0.2,0.1,0.2,1.65]
["Industry/Workshop",1.6,0.2,0.1,0.1,1,0]
[]
["Traveling Habit data"]
[null,null,"Travel method distribution",null,null,null,null,null,null,null,null,null,null,null,"Other Travel Data"]
[null,null,"Work",null,null,"Service",null,null,"Private errand",null,null,"Other",null,null,"Traveling speeds at road",null,"Average distance",null,"# passengers",null,"Public Transport"]
["Oslo",null,"Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","% below 50 km/h","% above 50 km/h","Public\nTransport","Car","Public\nTransport","Car","% using track"]
[null,"Residential individual housing",0.19,0.47,0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Residential apartment building",{"$f":"C24","v":0.19},{"$f":"D24","v":0.47},0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Office building",0.19,0.47,0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,{"$f":"O25","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Kindergarten",{"$f":"C26","v":0.19},{"$f":"D26","v":0.47},0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"School",{"$f":"C27","v":0.19},{"$f":"D27","v":0.47},{"$f":"E27","v":0.34},{"$f":"F27","v":0.19},{"$f":"G27","v":0.28999999999999998},{"$f":"H27","v":0.52},{"$f":"I27","v":0.42},{"$f":"J27","v":0.21},{"$f":"K27","v":0.37},{"$f":"L27","v":0.43},{"$f":"M27","v":0.26},{"$f":"N27","v":0.31},0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"University/Collage",0.19,0.47,0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Hospital",0.19,0.47,0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Nursing home",0.19,0.47,0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Hotel",0.19,0.47,0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Sports Facility",0.19,0.47,0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Comercial building",0.19,0.47,0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,{"$f":"O33","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Cultural building",{"$f":"C34","v":0.19},{"$f":"D34","v":0.47},0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Industry/Workshop",{"$f":"C33","v":0.19},{"$f":"D33","v":0.47},0.34,0.19,0.28999999999999998,0.52,0.42,0.21,0.37,0.43,0.26,0.31,{"$f":"O35","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[]
["Oslo, Groruddalen",null,"Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","% below 50 km/h","% above 50 km/h","Public\nTransport","Car","Public\nTransport","Car","% using track"]
[null,"Residential individual housing",0.11,0.5,0.39,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Residential apartment building",{"$f":"C39","v":0.11},{"$f":"D39","v":0.5},{"$f":"E39","v":0.39},{"$f":"F39","v":0.08},{"$f":"G39","v":0.23},{"$f":"H39","v":0.69},{"$f":"I39","v":0.33},{"$f":"J39","v":0.22},{"$f":"K39","v":0.45},{"$f":"L39","v":0.39},{"$f":"M39","v":0.28000000000000003},{"$f":"N39","v":0.33},0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Office building",0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,{"$f":"O40","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Kindergarten",{"$f":"C41","v":0.09},{"$f":"D41","v":0.3},{"$f":"E41","v":0.61},{"$f":"F41","v":0.08},{"$f":"G41","v":0.23},{"$f":"H41","v":0.69},{"$f":"I41","v":0.33},{"$f":"J41","v":0.22},{"$f":"K41","v":0.45},{"$f":"L41","v":0.39},{"$f":"M41","v":0.28000000000000003},{"$f":"N41","v":0.33},0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"School",{"$f":"C42","v":0.09},0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"University/Collage",0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Hospital",0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Nursing home",0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Hotel",0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Sports Facility",0.09,0.3,0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Comercial building",{"$f":"C39","v":0.11},{"$f":"D39","v":0.5},0.39,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,{"$f":"O48","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Cultural building",{"$f":"C49","v":0.11},{"$f":"D49","v":0.5},{"$f":"E49","v":0.39},{"$f":"F49","v":0.08},{"$f":"G49","v":0.23},{"$f":"H49","v":0.69},{"$f":"I49","v":0.33},{"$f":"J49","v":0.22},{"$f":"K49","v":0.45},{"$f":"L49","v":0.39},{"$f":"M49","v":0.28000000000000003},{"$f":"N49","v":0.33},0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Industry/Workshop",{"$f":"C48","v":0.09},{"$f":"D48","v":0.3},0.61,0.08,0.23,0.69,0.33,0.22,0.45,0.39,0.28000000000000003,0.33,{"$f":"O50","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[]
["Oslo, Groruddalen knutepunkt",null,"Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","% below 50 km/h","% above 50 km/h","Public\nTransport","Car","Public\nTransport","Car","% using track"]
[null,"Residential individual housing",0.2,0.5,0.3,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.44,0.28000000000000003,0.28000000000000003,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Residential apartment building",{"$f":"C54","v":0.2},{"$f":"D54","v":0.5},{"$f":"E54","v":0.3},{"$f":"F54","v":0.17},{"$f":"G54","v":0.28000000000000003},{"$f":"H54","v":0.55000000000000004},{"$f":"I54","v":0.46},{"$f":"J54","v":0.22},{"$f":"K54","v":0.32},{"$f":"L54","v":0.44},{"$f":"M54","v":0.28000000000000003},{"$f":"N54","v":0.28000000000000003},0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Office building",0.15,0.37,0.48,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.43,0.25,0.32,{"$f":"O55","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Kindergarten",{"$f":"C56","v":0.15},{"$f":"D56","v":0.37},{"$f":"E56","v":0.48},{"$f":"F56","v":0.17},{"$f":"G56","v":0.28000000000000003},{"$f":"H56","v":0.55000000000000004},{"$f":"I56","v":0.46},{"$f":"J56","v":0.22},{"$f":"K56","v":0.32},{"$f":"L56","v":0.43},{"$f":"M56","v":0.25},{"$f":"N56","v":0.32},0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"School",{"$f":"C57","v":0.15},0.37,0.48,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.43,0.25,0.32,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"University/Collage",0.15,0.37,0.48,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.43,0.25,0.32,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Hospital",0.15,0.37,0.48,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.43,0.25,0.32,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Nursing home",0.15,0.37,0.48,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.43,0.25,0.32,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Hotel",0.15,0.37,0.48,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.43,0.25,0.32,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Sports Facility",0.15,0.37,0.48,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.43,0.25,0.32,0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Comercial building",{"$f":"C54","v":0.2},{"$f":"D54","v":0.5},0.3,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.44,0.28000000000000003,0.28000000000000003,{"$f":"O63","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Cultural building",{"$f":"C64","v":0.2},{"$f":"D64","v":0.5},{"$f":"E64","v":0.3},{"$f":"F64","v":0.17},{"$f":"G64","v":0.28000000000000003},{"$f":"H64","v":0.55000000000000004},{"$f":"I64","v":0.46},{"$f":"J64","v":0.22},{"$f":"K64","v":0.32},{"$f":"L64","v":0.44},{"$f":"M64","v":0.28000000000000003},{"$f":"N64","v":0.28000000000000003},0.5,0.5,13.8,16,19.399999999999999,1.3,0.6]
[null,"Industry/Workshop",{"$f":"C63","v":0.15},{"$f":"D63","v":0.37},0.48,0.17,0.28000000000000003,0.55000000000000004,0.46,0.22,0.32,0.43,0.25,0.32,{"$f":"O65","v":0.5},0.5,13.8,16,19.399999999999999,1.3,0.6]
[]
["Bergen Kommune",null,"Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","% below 50 km/h","% above 50 km/h","Public\nTransport","Car","Public\nTransport","Car","% using track"]
[null,"Residential individual housing",0.27,0.25,0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,1.3,0.2]
[null,"Residential apartment building",{"$f":"C69","v":0.27},{"$f":"D69","v":0.25},0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,1.3,0.2]
[null,"Office building",{"$f":"C70","v":0.27},{"$f":"D70","v":0.25},0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,{"$f":"O70","v":0.6},0.4,12.3,12.9,15,1.3,0.2]
[null,"Kindergarten",{"$f":"C71","v":0.27},{"$f":"D71","v":0.25},0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,{"$f":"T71","v":1.3},0.2]
[null,"School",{"$f":"C72","v":0.27},0.25,0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,{"$f":"T72","v":1.3},0.2]
[null,"University/Collage",0.27,0.25,0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,{"$f":"T73","v":1.3},0.2]
[null,"Hospital",0.27,0.25,0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,{"$f":"T74","v":1.3},0.2]
[null,"Nursing home",0.27,0.25,0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,{"$f":"T75","v":1.3},0.2]
[null,"Hotel",0.27,0.25,0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,{"$f":"T76","v":1.3},0.2]
[null,"Sports Facility",0.27,0.25,0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,{"$f":"T77","v":1.3},0.2]
[null,"Comercial building",{"$f":"C69","v":0.27},{"$f":"D69","v":0.25},0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,{"$f":"O78","v":0.6},0.4,12.3,12.9,15,1.3,0.2]
[null,"Cultural building",{"$f":"C79","v":0.27},{"$f":"D79","v":0.25},0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.9,15,1.3,0.2]
[null,"Industry/Workshop",{"$f":"C78","v":0.27},{"$f":"D78","v":0.25},0.48,0.09,0.12,0.79,0.41,0.11,0.48,0.32,0.1,0.57999999999999996,{"$f":"O80","v":0.6},0.4,12.3,12.9,15,1.3,0.2]
[]
["Bergen Sentrum",null,"Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","% below 50 km/h","% above 50 km/h","Public\nTransport","Car","Public\nTransport","Car","% using track"]
[null,"Residential individual housing",0.4,0.21,0.39,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Residential apartment building",{"$f":"C84","v":0.4},{"$f":"D84","v":0.21},0.39,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Office building",0.28000000000000003,0.28000000000000003,0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,{"$f":"O85","v":0.6},0.4,12.3,12.3,15,1.3,0.2]
[null,"Kindergarten",{"$f":"C86","v":0.28000000000000003},{"$f":"D86","v":0.28000000000000003},0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"School",{"$f":"C87","v":0.28000000000000003},0.28000000000000003,0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"University/Collage",0.28000000000000003,0.28000000000000003,0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Hospital",0.28000000000000003,0.28000000000000003,0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Nursing home",0.28000000000000003,0.28000000000000003,0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Hotel",0.28000000000000003,0.28000000000000003,0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Sports Facility",0.28000000000000003,0.28000000000000003,0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Comercial building",{"$f":"C84","v":0.4},{"$f":"D84","v":0.21},0.39,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,{"$f":"O93","v":0.6},0.4,12.3,12.3,15,1.3,0.2]
[null,"Cultural building",{"$f":"C94","v":0.4},{"$f":"D94","v":0.21},0.39,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Industry/Workshop",{"$f":"C93","v":0.28000000000000003},{"$f":"D93","v":0.28000000000000003},0.79,0.09,0.12,0.79,0.51,0.09,0.4,0.32,0.1,0.57999999999999996,{"$f":"O95","v":0.6},0.4,12.3,12.3,15,1.3,0.2]
[]
["Bergen Kommune, utenfor sentrum",null,"Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","Walk/bike","Public transport","Car","% below 50 km/h","% above 50 km/h","Public\nTransport","Car","Public\nTransport","Car","% using track"]
[null,"Residential individual housing",0.12,0.16,0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Residential apartment building",{"$f":"C99","v":0.12},{"$f":"D99","v":0.16},0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Office building",{"$f":"C100","v":0.12},{"$f":"D100","v":0.16},0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,{"$f":"O100","v":0.6},0.4,12.3,12.3,15,1.3,0.2]
[null,"Kindergarten",{"$f":"C101","v":0.12},{"$f":"D101","v":0.16},0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"School",{"$f":"C102","v":0.12},0.16,0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"University/Collage",0.12,0.16,0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Hospital",0.12,0.16,0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Nursing home",0.12,0.16,0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Hotel",0.12,0.16,0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Sports Facility",0.12,0.16,0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Comercial building",{"$f":"C99","v":0.12},{"$f":"D99","v":0.16},0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,{"$f":"O108","v":0.6},0.4,12.3,12.3,15,1.3,0.2]
[null,"Cultural building",{"$f":"C109","v":0.12},{"$f":"D109","v":0.16},0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,0.6,0.4,12.3,12.3,15,1.3,0.2]
[null,"Industry/Workshop",{"$f":"C108","v":0.12},{"$f":"D108","v":0.16},0.72,0.09,0.12,0.79,0.17,7.0000000000000007E-2,0.76,0.32,0.1,0.57999999999999996,{"$f":"O110","v":0.6},0.4,12.3,12.3,15,1.3,0.2]

{"sheet":"Test","index":3,"n_rows":56,"n_cols":50,"rows_kept":56,"cut":false,"hidden":true,"merged":[]}
[null,"Work","Service","Private errand","Utside Service","Goods transport","Other",null,"Walk/bike","Work","Service","Private errand","Utside Service","Goods transport","Other",null,"Walk/bike","Work","Service","Private errand","Utside Service","Goods transport","Other",null,"Walk/bike","Work","Service","Private errand","Utside Service","Goods transport","Other",null,"Walk/bike","Work","Service","Private errand","Utside Service","Goods transport","Other",null,"Walk/bike","Work","Service","Private errand","Utside Service","Goods transport","Other"]
["Residential individual housing",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,16286580.528409088]
["Residential apartment building",3039.2000000000003,379.90000000000003,3799,6458.3,379.90000000000003,0,null,null,334.31200000000001,30.392000000000003,1253.67,516.66399999999999,0,0,null,null,null,null,null,null,null,null,null,null,1056.1600000000001,112.21700000000001,3036.46,1907.6889999999999,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0]
["Office building",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,262.56,111.58800000000001,100.64800000000001,18.598000000000003,0,672.70059999999989,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,7565350.8647832153]
["Kindergarten",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,23.040000000000003,9.7919999999999998,8.8320000000000025,1.6320000000000003,0,207.8964,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,2608157.3106060605]
["School",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,28.799999999999997,12.24,11.040000000000001,2.04,0,314.072,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0]
["University/Collage",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0]
["Hospital",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,39.119999999999997,16.626000000000001,14.996,2.7710000000000004,0,123.84,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
["Nursing home",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
["Hotel",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
["Sports Facility",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,3.12,1.3260000000000001,1.1960000000000002,0.22100000000000003,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
["Comercial building",96,12,6,6,60,330,null,null,10.56,0.96,1.98,0.48,0,128.70000000000002,null,null,null,null,null,null,null,null,null,null,256,27.200000000000003,36.800000000000004,13.600000000000001,0,9982.5,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
["Cultural building",8,3,1,0.5,1,165,null,null,0.88,0.24,0.33,0.04,0,64.350000000000009,null,null,null,null,null,null,null,null,null,null,16,5.1000000000000005,4.6000000000000005,0.85000000000000009,0,3005.64,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
["Industry/Workshop",0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[]
[null,null,null,null,null,null,null,null,"Public",0,0,0,0,0,0,null,"Public",null,null,null,null,null,null,null,"Public",0,0,0,0,0,0,null,"Bus",0,0,0,0,0,0,null,"Bus",0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,1519.6000000000001,87.37700000000001,835.78,1485.4090000000001,0,0,null,null,null,null,null,null,null,null,null,null,2640.4,184.82800000000003,1452.22,3142.076,0,0,null,null,3400.503496503497,195.52895104895106,1870.2769230769231,3323.992167832168,0,0,null,null,2677896.5034965039,153979.04895104896,1472843.076923077,2617643.8321678322,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,647.64800000000002,183.792,48.136000000000003,30.632000000000005,0,391.10499999999996,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,56.832000000000008,16.128,4.2240000000000011,2.6880000000000006,0,120.87,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,71.039999999999992,20.160000000000004,5.28,3.3600000000000003,0,182.6,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,96.496000000000009,27.384,7.1720000000000006,4.5640000000000009,0,72,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,7.6959999999999997,2.1840000000000002,0.57200000000000006,0.36400000000000005,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,48,2.7600000000000002,1.32,1.3800000000000001,0,92.4,null,null,null,null,null,null,null,null,null,null,640,44.800000000000004,17.600000000000001,22.400000000000002,0,6352.5000000000009,null,null,132.54713286713286,6.1762237762237771,2.953846153846154,3.0881118881118885,0,279.87692307692311,null,null,104380.86713286713,4863.7762237762245,2326.1538461538462,2431.8881118881122,0,220403.07692307694]
[null,null,null,null,null,null,null,null,null,4,0.69000000000000006,0.22,0.115,0,46.2,null,null,null,null,null,null,null,null,null,null,40,8.4,2.2000000000000002,1.4000000000000001,0,1912.6800000000003,null,null,8.9510489510489517,1.5440559440559443,0.49230769230769228,0.25734265734265732,0,103.38461538461539,null,null,7048.9510489510494,1215.9440559440561,387.69230769230768,202.65734265734264,0,81415.384615384624]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[]
[null,null,null,null,null,null,null,null,"Car",0,0,0,0,0,0,null,"Car",null,null,null,null,null,null,null,"Car",0,0,0,0,0,0,null,"Rail",0,0,0,0,0,0,null,"Rail",0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,1185.2880000000002,262.13100000000003,1709.55,4456.2269999999999,379.90000000000003,0,null,null,null,null,null,null,null,null,null,null,1584.24,363.05500000000006,2112.3200000000002,6171.9349999999995,660.1,0,null,null,6630.9818181818182,381.28145454545455,3647.0399999999995,6481.7847272727267,0,0,null,null,79571.781818181815,4575.3774545454544,43764.479999999996,77781.416727272721,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,840.19200000000001,361.02000000000004,70.016000000000005,60.170000000000009,218.8,500.61439999999999,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,73.728000000000009,31.68,6.144000000000001,5.2800000000000011,19.200000000000003,154.71360000000001,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,92.16,39.6,7.68,6.6000000000000005,24,233.72800000000001,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,125.184,53.790000000000006,10.432,8.9650000000000016,32.6,92.16,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,9.984,4.29,0.83200000000000007,0.71500000000000008,2.6,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,37.44,8.2799999999999994,2.7,4.1399999999999997,60,108.9,null,null,22.463999999999999,null,null,null,null,65.34,null,null,384,88,25.6,44,800,6352.5000000000009,null,null,258.46690909090904,12.043636363636365,5.76,6.0218181818181824,0,545.76,null,null,3101.6029090909087,144.52363636363637,69.12,72.261818181818185,0,6549.12]
[null,null,null,null,null,null,null,null,null,3.12,2.0699999999999998,0.45,0.34499999999999997,1,54.45,null,null,3.12,null,null,null,null,54.45,null,null,24,16.5,3.2,2.75,10,1912.6800000000003,null,null,17.454545454545453,3.0109090909090912,0.95999999999999985,0.50181818181818172,0,201.6,null,null,209.45454545454544,36.130909090909093,11.519999999999998,6.0218181818181806,0,2419.1999999999998]
[null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,null,null,null,null,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Car",17420.141818181819,3852.5313636363635,25125.20454545454,65493.033181818173,5583.378787878788,0,null,"Car",2482370.209090909,548985.71931818186,3580341.6477272725,9332757.2284090891,2247309.9621212124,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330.15272727272725,121.69090909090907,39.68181818181818,60.845454545454537,881.81818181818176,960.3,null,null,47046.763636363627,17340.954545454544,5654.6590909090901,8670.4772727272721,354931.81818181812,136842.75]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45.854545454545452,30.422727272727268,6.6136363636363633,5.0704545454545444,14.696969696969695,800.25,null,null,6534.272727272727,4335.238636363636,942.44318181818176,722.53977272727252,5915.5303030303021,114035.625]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,null,null,0,0,0,0,0,0]

{"sheet":"EnergyPerformanceData","index":4,"n_rows":131,"n_cols":15,"rows_kept":131,"cut":false,"hidden":true,"merged":[]}
["Building energy perfromance data [kWh/m2]",{"$f":"COUNTA(A2:A131)","v":130},null,null,null,null,"Infrastructure Energy performance data",null,null,"Klimasone"]
["Residential individual housing","Heating","Hot Water","Cooling","Electric",null,"Outdoor lighting","kWh/unit",null,"Klimasone","DUT","Mean T","Heating days","degree days","Rel degree days"]
["Passivhouse",15.2,29.8,0,33,null,"High efficicency",160,null,"1. Sør-Norge, innland",-21.4,5.0999999999999996,250,4051,1]
["Low energy",30,29.8,0,33,null,"Low efficiency",550,null,"2. Sør-Norge, kyst",-14.2,7.1,237,3179,0.78]
["TEK 10",57.9,29.8,0,32.9,null,"Manual",null,null,"3. Sør-Norge, høyfjell",-28.3,2.2999999999999998,277,5101,1.26]
["TEK 07",57.9,29.8,0,32.9,null,"Snow Melting","kWh/m2",null,"4. Midt-Norge, kyst",-15.6,5.4,265,3763,0.93]
["TEK 97",84.2,29.8,0,41.9,null,"High efficicency",100,null,"5. Midt-Norge, innland",-23.9,3,274,4772,1.18]
["TEK 87",164.8,29.8,0,34.700000000000003,null,"Low efficiency",350,null,"6. Nord-Norge, kyst",-13.9,3.8,286,4329,1.07]
["TEK 69",169,29.8,0,34.700000000000003,null,"Manual",null,null,"7. Finnmark og innland Troms",-24.5,0.7,319,5766,1.42]
["TEK 49",204.8,29.8,0,34.700000000000003]
["Older",258.89999999999998,29.8,0,34.700000000000003]
["Residential apartment building","Heating","Hot Water","Cooling","Electric"]
["Passivhouse",15.2,29.8,0,33]
["Low energy",30,29.8,0,33]
["TEK 10",36.200000000000003,29.8,0,33.5]
["TEK 07",36.200000000000003,29.8,0,33.5]
["TEK 97",48.2,29.8,0,42.7]
["TEK 87",99.7,29.8,0,35.1]
["TEK 69",97.2,29.8,0,35.1]
["TEK 49",170.7,29.8,0,35.1]
["Older",190.9,29.8,0,35.200000000000003]
["Office building","Heating","Hot Water","Cooling","Electric"]
["Passivhouse",20,5,9,44]
["Low energy",23.200000000000003,5,9.8000000000000007,63.2]
["TEK 10",40.200000000000003,5,15.7,75.2]
["TEK 07",59.400000000000006,5,18.8,84]
["TEK 97",78.3,5,20.8,100.30000000000001]
["TEK 87",96.4,5,21.4,127.80000000000001]
["TEK 69",162.6,5,11.4,107.8]
["TEK 49",173.5,5,0,92.4]
["Older",188.7,5,0,82.8]
["Kindergarten","Heating","Hot Water","Cooling","Electric"]
["Passivhouse",28,10,5,29]
["Low energy",48.4,10,0,31.599999999999998]
["TEK 10",80.2,10,0,41.2]
["TEK 07",100.6,10,0,49.2]
["TEK 97",129.5,10,0,66.2]
["TEK 87",163.19999999999999,10,0,90.2]
["TEK 69",287,10,0,72.8]
["TEK 49",339.6,10,0,45.900000000000006]
["Older",381.1,10,0,45.900000000000006]
["School","Heating","Hot Water","Cooling","Electric"]
["Passivhouse",20.2,9.8000000000000007,5,30]
["Low energy",30,9.8000000000000007,0,37.700000000000003]
["TEK 10",50.1,9.8000000000000007,0,51.199999999999996]
["TEK 07",73.400000000000006,9.8000000000000007,0,59.800000000000004]
["TEK 97",104.1,9.8000000000000007,0,78.300000000000011]
["TEK 87",127.2,9.8000000000000007,0,103.30000000000001]
["TEK 69",196.6,9.8000000000000007,0,77.900000000000006]
["TEK 49",208.3,9.8000000000000007,0,54.699999999999996]
["Older",227.3,9.8000000000000007,0,54.699999999999996]
["University/Collage","Heating","Hot Water","Cooling","Electric"]
["Passivhouse"]
["Low energy",21.299999999999997,5,10.8,68.099999999999994]
["TEK 10",39.4,5,19.600000000000001,79.8]
["TEK 07",63.1,5,23.4,89.8]
["TEK 97",83,5,25.8,110.2]
["TEK 87",102.5,5,26.6,138.80000000000001]
["TEK 69",174,5,15.1,115.19999999999999]
["TEK 49",167.1,5,0,82.7]
["Older",182.2,5,0,82.8]
["Hospital","Heating","Hot Water","Cooling","Electric"]
["Passivhouse"]
["Low energy",54.699999999999996,29.8,21,112.10000000000001]
["TEK 10",62.9,29.8,30.5,131.60000000000002]
["TEK 07",114.8,29.8,37.5,151.69999999999999]
["TEK 97",136.4,29.8,42,192.7]
["TEK 87",144.30000000000001,29.8,43.6,247.10000000000002]
["TEK 69",181.4,29.8,19.600000000000001,186.8]
["TEK 49",134.6,29.8,0,135.39999999999998]
["Older",149.30000000000001,29.8,0,135.6]
["Nursing home","Heating","Hot Water","Cooling","Electric"]
["Passivhouse",20.2,29.8,11,70]
["Low energy",38.6,29.8,0,76.5]
["TEK 10",59.2,29.8,0,100]
["TEK 07",99,29.8,0,118.80000000000001]
["TEK 97",132.69999999999999,29.8,0,154.80000000000001]
["TEK 87",149.1,29.8,0,207.70000000000002]
["TEK 69",177.10000000000002,29.8,0,147.6]
["TEK 49",169.9,29.8,0,112.29999999999998]
["Older",188.5,29.8,0,112.4]
["Hotel","Heating","Hot Water","Cooling","Electric"]
["Passivhouse"]
["Low energy",44,29.8,11.9,56.199999999999996]
["TEK 10",70.099999999999994,29.8,20.5,75.099999999999994]
["TEK 07",100.89999999999999,29.8,25.5,91.899999999999991]
["TEK 97",130.30000000000001,29.8,28.6,118.2]
["TEK 87",137.30000000000001,29.8,29.7,167.9]
["TEK 69",194,29.8,14.9,132.1]
["TEK 49",187.5,29.8,0,94.699999999999989]
["Older",206.3,29.8,0,94.8]
["Sports Facility","Heating","Hot Water","Cooling","Electric"]
["Passivhouse",20,49,6,26,101]
["Low energy",49.2,49,0,28.9]
["TEK 10",76,49,0,38.200000000000003]
["TEK 07",96.699999999999989,49,0,46.1]
["TEK 97",141.19999999999999,49,0,63.000000000000007]
["TEK 87",170.7,49,0,86.8]
["TEK 69",301.5,49,0,78.3]
["TEK 49",295.8,49,0,42.7]
["Older",326.3,49,0,42.7]
["Comercial building","Heating","Hot Water","Cooling","Electric"]
["Passivhouse",25.5,10.5,22,65]
["Low energy",30.4,10.5,18.7,72.8]
["TEK 10",73,10.5,34.1,92.3]
["TEK 07",117.5,10.5,40.799999999999997,112]
["TEK 97",139.1,10.5,45,148.19999999999999]
["TEK 87",140.60000000000002,10.5,46.4,209.6]
["TEK 69",137.80000000000001,10.5,12.7,138]
["TEK 49",141.9,10.5,0,110.10000000000001]
["Older",156.80000000000001,10.5,0,110.2]
["Cultural building","Heating","Hot Water","Cooling","Electric"]
["Passivhouse",25,10,8,29]
["Low energy",39.400000000000006,10,6.7,32.299999999999997]
["TEK 10",79.7,10,16.399999999999999,43.999999999999993]
["TEK 07",103.1,10,19.399999999999999,52.699999999999996]
["TEK 97",130.69999999999999,10,21.4,70.5]
["TEK 87",149.9,10,22.1,96.700000000000017]
["TEK 69",210,10,10.4,71.2]
["TEK 49",231.8,10,0,47.4]
["Older",252.7,10,0,47.4]
["Industry/Workshop","Heating","Hot Water","Cooling","Electric"]
["Passivhouse"]
["Low energy",48.099999999999994,10,5.7,47.9]
["TEK 10",78.199999999999989,10,15,60.4]
["TEK 07",99.1,10,17.7,68]
["TEK 97",128.19999999999999,10,19.5,83.5]
["TEK 87",161.30000000000001,10,20.2,105.30000000000001]
["TEK 69",313.5,10,16.100000000000001,97.600000000000009]
["TEK 49",303.60000000000002,10,0,60.1]
["Older",333.2,10,0,60.1]

{"sheet":"LocalEnergySupplyData","index":5,"n_rows":58,"n_cols":8,"rows_kept":58,"cut":false,"hidden":true,"merged":[[14,1,14,4],[14,5,14,7]]}
["Emission Factors","Emissions [gCO2/kWh]",null,null,null,"Tall må oppdateres og sjekkes"]
["Energy Sources","Indirect","upstream","Total"]
["Electricity",17,0,123]
["Solar Thermal",0,0,{"$f":"SUM(B4:C4)","v":0}]
["Firewood",14,0,14]
["Wood Chips",14,0,14]
["Pellets",25,0,25]
["Bio-oil",25,0,25]
["Bio-gas",10,0,10]
["Waste",138,0,138]
["Fossile oil",50,265,315]
["LPG",70,234,304]
["Natural Gas",53,202,255]
[]
[null,"Efficiency",null,null,null,"CO2 factor"]
["Heating","Production-\nEfficiency","Distribution-\nEfficiency","Control-\nEfficiency","Total\nEfficiency","Source","Efficiency","Total"]
["Electric heater",0.99,0.99,0.9,{"$f":"B17*C17*D17","v":0.88209000000000004},"Electricity",1,{"$f":"OFFSET($A$3,MATCH(F17,emissionSourcesRange,0)-1,3)/G17","v":123}]
["Electric boiler",0.98,0.95,0.92,{"$f":"B18*C18*D18","v":0.85651999999999995},"Electricity",1,123]
["Solar collector",1,0.95,0.95,0.90249999999999997,"Solar Thermal",1,0]
["Heat pump",2.5499999999999998,0.95,0.93,2.2529249999999998,"Electricity",1,123]
["Wood chip boiler",0.85,0.97,0.9,{"$f":"B21*C21*D21","v":0.74204999999999999},"Wood Chips",1,14]
["Pellets boiler",0.85,0.97499999999999998,0.9,0.74587499999999995,"Pellets",1,25]
["Wood-burning Stove",0.8,1,0.8,0.64000000000000012,"Firewood",1,14]
["Bio-oil boiler",0.85,0.95,0.94,0.75905,"Bio-oil",1,25]
["Oil boiler",0.85,0.95,0.95,0.76712499999999995,"Fossile oil",1,315]
["LPG boiler",0.95,0.95,0.95,0.85737499999999989,"LPG",1,304]
["District Heating",0.98,0.95,0.93,0.86582999999999999]
[]
["Hot Water"]
["Electric water heater",0.99,0.6,0.98,{"$f":"B30*C30*D30","v":0.58211999999999997},"Electricity",1,{"$f":"OFFSET($A$3,MATCH(F30,emissionSourcesRange,0)-1,3)/G30","v":123}]
["Electric bolier",0.98,0.6,0.92,{"$f":"B31*C31*D31","v":0.54096},"Electricity",1,123]
["Solar collector",1,0.6,0.95,{"$f":"B32*C32*D32","v":0.56999999999999995},"Solar Thermal",1,0]
["Heat Pump",2.5499999999999998,0.6,0.93,1.4228999999999998,"Electricity",1,123]
["Wood chip boiler",0.85,0.6,0.9,{"$f":"B34*C34*D34","v":0.45900000000000002},"Wood Chips",1,14]
["Pellets boiler",0.85,0.6,0.9,0.45900000000000002,"Pellets",1,25]
["Bio-oil boiler",0.85,0.6,0.94,{"$f":"B36*C36*D36","v":0.47939999999999999},"Bio-oil",1,25]
["Oil boiler",0.85,0.6,0.95,0.48449999999999999,"Fossile oil",1,315]
["LPG boiler",0.95,0.6,0.95,0.54149999999999998,"LPG",1,304]
["District Heating",0.98,0.6,0.93,0.54683999999999999]
[]
["Cooling"]
["Local Chiller",2.4500000000000002,1,1,{"$f":"B42*C42*D42","v":2.4500000000000002},"Electricity",1,{"$f":"OFFSET($A$3,MATCH(F42,emissionSourcesRange,0)-1,3)/G42","v":123}]
["District cooling",2.5,0.95,0.93,2.2087500000000002,"Electricity",1,{"$f":"OFFSET($A$3,MATCH(F43,emissionSourcesRange,0)-1,3)/G43","v":123}]
[]
["Electric"]
["Electric consumption",1,1,1,{"$f":"B46*C46*D46","v":1},"Electricity",1,{"$f":"OFFSET($A$3,MATCH(F46,emissionSourcesRange,0)-1,3)/G46","v":123}]
[]
["Local energy plant sources"]
["Electricity",null,null,null,null,"Electricity",1,{"$f":"OFFSET($A$3,MATCH(F49,emissionSourcesRange,0)-1,3)/G49","v":123}]
["Sun",null,null,null,null,"Solar Thermal",1,{"$f":"OFFSET($A$3,MATCH(F50,emissionSourcesRange,0)-1,3)/G50","v":0}]
["Surplus Heat"]
["Waste Incineration",null,null,null,null,"Waste",1,{"$f":"OFFSET($A$3,MATCH(F52,emissionSourcesRange,0)-1,3)/G52","v":138}]
["Wood Chips",null,null,null,null,"Wood Chips",1,14]
["Pellets",null,null,null,null,"Pellets",1,25]
["Bio-oil",null,null,null,null,"Bio-oil",1,25]
["Bio-gas",null,null,null,null,"Bio-gas",1,10]
["Fossile Oil",null,null,null,null,"Fossile oil",1,315]
["LPG",null,null,null,null,"LPG",1,304]

{"sheet":"Lists","index":6,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":true,"merged":[]}
["Building Categories","Building performance data","Energy Certificates","Ownership","PV input","Energy technology"]
["Residential individual housing","Passivhouse","A","Public","Auto","Fossile "]
["Residential apartment building","Low energy","B","Private","Manual","Renewable/electric"]
["Office building","TEK 10","C","Housing cooperative"]
["Kindergarten","TEK 07","D"]
["School","TEK 97","E"]
["University/Collage","TEK 87","F"]
["Hospital","TEK 69","G"]
["Nursing home","TEK 49"]
["Hotel","Older"]
["Sports Facility","Simulation"]
["Comercial building","Measurements"]
["Cultural building"]
["Industry/Workshop"]
[]
["Local energy plant list"]
["CHP"]
["Solar PV"]
["Solar Thermal"]
["Boiler"]
["Heat Pump"]
["Direct connection"]
[]
["Goal Catergory List","Unit List","Comparison"]
["Energy Consumption","Absolute","Absolute"]
["Energy Generation","/m2 BRA","% Increase"]
["Mismatch","/inhabitant","% Reduction"]
[null,"/person"]
["Mobility"]
["Carbon Emission"]
[]
["Goal List","# KPIs","CO2-reduction","Increased use of renewable energy","Increased energy efficiency","Increased use of local energy sources","Green mobility"]
["CO2-reduction",null,{"$f":"COUNTA(C34:C43)","v":3},{"$f":"COUNTA(D34:D41)","v":7},{"$f":"COUNTA(E34:E42)","v":3},{"$f":"COUNTA(F34:F42)","v":7},{"$f":"COUNTA(G34:G41)","v":2}]
["Increased use of renewable energy",null,"CO2 emissions","% of different kinds of RES in district heating","Energy Use","Installed capacity of RES","Modal Split"]
["Increased energy efficiency",null,"# fossil free construction sites","# fossile free construction sites","% of buildings with Energy Certificate at each of the grades","Generated energy by RES","# filling stations with RES fuel for public access"]
["Increased use of local energy sources",null,"Number of registered oil tanks","Installed capacity of RES","% of buildings with measurement values for energy performance","Buildings with installed Solar Energy System"]
["Green mobility",null,null,"Generated energy by RES",null,"Use of secondary heat"]
[null,null,null,"Buildings with installed Solar Energy System",null,"Buildings connected to district thermal energy "]
[null,null,null,"Buildings connected to district thermal energy ",null,"Peak Load Production"]
[null,null,null,"Number of registered oil tanks",null,"Energy Storage"]
[]
[]
[]
[]
["Location List"]
["Oslo og Akershus"]
["Bergen, Trondheim og Stavanger area"]
["Other Cities"]

{"sheet":"KPIResults","index":7,"n_rows":193,"n_cols":7,"rows_kept":193,"cut":false,"hidden":false,"merged":[]}
["Scenario",null,null,null,null,null,"Initial"]
[]
["Key Data",null,"Category","Sub-Category","Sectors","Unit"]
["Year",null,null,null,null,null,2015]
["Population",null,null,null,null,"#",280]
["Number of jobs",null,null,null,null,"#",150]
["Other Users",null,null,null,null,"#",105]
["Building area",null,null,null,"Total","m2",25000]
[null,null,null,null,"Residential buildings","m2",20000]
[null,null,null,null,"Public buildings","m2",0]
[null,null,null,null,"Private buildings","m2",5000]
["Number of buildings",null,null,null,"Total","#",2]
[null,null,null,null,"Residential buildings","#",1]
[null,null,null,null,"Public buildings","#",0]
[null,null,null,null,"Private buildings","#",1]
[]
["KPI",null,"Category","Sub-Category","Sectors","Unit"]
["Energy Use",null,"Total","Total","Total","kWh",4867800.2801773604]
[null,null,null,null,"Residential buildings","kWh",3986384.1886650929]
[null,null,null,null,"Public buildings","kWh",0]
[null,null,null,null,"Private buildings","kWh",802715.48907449609]
[null,null,null,null,"Infrastructure","kWh",78700.602437771449]
[null,null,"Electric","Total","Total","kWh",4867800.2801773604]
[null,null,null,null,"Residential buildings","kWh",3986384.1886650929]
[null,null,null,null,"Public buildings","kWh",0]
[null,null,null,null,"Private buildings","kWh",802715.48907449609]
[null,null,null,null,"Infrastructure","kWh",78700.602437771449]
[null,null,null,"Buildings","Total","kWh",4789099.6777395885]
[null,null,null,null,"Residential buildings","kWh",3986384.1886650929]
[null,null,null,null,"Public buildings","kWh",0]
[null,null,null,null,"Private buildings","kWh",802715.48907449609]
[null,null,null,"Infrastructure","Total","kWh",78700.602437771449]
[null,null,null,null,"Outdoor lighting","kWh",32000]
[null,null,null,null,"Transport","kWh",0]
[null,null,null,null,"Other","kWh",46700.602437771449]
[null,null,"Thermal","Total","Total","kWh",0]
[null,null,null,null,"Solar","kWh",0]
[null,null,null,null,"Biofuel","kWh",0]
[null,null,null,null,"Oil","kWh",0]
[null,null,null,null,"Gas","kWh",0]
[null,null,null,null,"District heating","kWh",0]
[null,null,null,"Residential Buildings","Total","kWh",0]
[null,null,null,null,"Solar","kWh",0]
[null,null,null,null,"Biofuel","kWh",0]
[null,null,null,null,"Oil","kWh",0]
[null,null,null,null,"Gas","kWh",0]
[null,null,null,null,"District heating","kWh",0]
[null,null,null,"Public Buildings","Total","kWh",0]
[null,null,null,null,"Solar","kWh",0]
[null,null,null,null,"Biofuel","kWh",0]
[null,null,null,null,"Oil","kWh",0]
[null,null,null,null,"Gas","kWh",0]
[null,null,null,null,"District heating","kWh",0]
[null,null,null,"Private Buildings","Total","kWh",0]
[null,null,null,null,"Solar","kWh",0]
[null,null,null,null,"Biofuel","kWh",0]
[null,null,null,null,"Oil","kWh",0]
[null,null,null,null,"Gas","kWh",0]
[null,null,null,null,"District heating","kWh",0]
[null,null,null,"Infrastructure","Total","kWh",0]
[null,null,null,null,"Solar","kWh",0]
[null,null,null,null,"Biofuel","kWh",0]
[null,null,null,null,"Oil","kWh",0]
[null,null,null,null,"Gas","kWh",0]
[null,null,null,null,"District heating","kWh",0]
["% of energy sources delivering to district heating system",null,"Total",null,null,"%",10.672000000000001]
[null,null,"Electricity",null,null,"%",30.728000000000002]
[null,null,"Surplus and Ambient Heat",null,null,"%",5.3720000000000008]
[null,null,"Solar",null,null,"%",0]
[null,null,"Biofuel",null,null,"%",5.3]
[null,null,"Waste",null,null,"%",57.599999999999994]
[null,null,"Oil",null,null,"%",0.2]
[null,null,"Gas",null,null,"%",0.8]
["% of buildings with Energy Certificate at each of the grades",null,"Total registered",null,null,"%",100]
[null,null,"Certificate A",null,null,"%",0]
[null,null,"Certificate B",null,null,"%",0]
[null,null,"Certificate C",null,null,"%",0]
[null,null,"Certificate D",null,null,"%",0]
[null,null,"Certificate E",null,null,"%",50]
[null,null,"Certificate F",null,null,"%",50]
[null,null,"Certificate G",null,null,"%",0]
[null,null,"Not registered",null,null,"%",0]
["% of buildings with measurement values for energy performance",null,null,null,"Total","%",0]
[null,null,null,null,"Residential buildings","%",0]
[null,null,null,null,"Public buildings","%",0]
[null,null,null,null,"Private buildings","%",0]
["Installed capacity of RES",null,"Total","Total",null,"kW",0]
[null,null,null,"Solar",null,"kW",0]
[null,null,null,"CHP Waste",null,"kW",0]
[null,null,null,"CHP Biomass",null,"kW",0]
[null,null,"Electric","Total",null,"kW",0]
[null,null,null,"Solar",null,"kW",0]
[null,null,null,"CHP Waste",null,"kW",0]
[null,null,null,"CHP Biomass",null,"kW",0]
[null,null,"Thermal","Total",null,"kW",0]
[null,null,null,"Solar",null,"kW",0]
[null,null,null,"CHP Waste",null,"kW",0]
[null,null,null,"CHP Biomass",null,"kW",0]
["Generated energy by RES",null,"Total","Total",null,"kWh",0]
[null,null,null,"Solar",null,"kWh",0]
[null,null,null,"CHP Waste",null,"kWh",0]
[null,null,null,"CHP Biomass",null,"kWh",0]
[null,null,"Electric","Total",null,"kWh",0]
[null,null,null,"Solar",null,"kWh",0]
[null,null,null,"CHP Waste",null,"kWh",0]
[null,null,null,"CHP Biomass",null,"kWh",0]
[null,null,"Thermal","Total",null,"kWh",0]
[null,null,null,"Solar",null,"kWh",0]
[null,null,null,"CHP Waste",null,"kWh",0]
[null,null,null,"CHP Biomass",null,"kWh",0]
["# of buildings with installed solar energy system",null,"Total",null,"Total","#",0]
[null,null,null,null,"Residential buildings","#",0]
[null,null,null,null,"Public buildings","#",0]
[null,null,null,null,"Private buildings","#",0]
[null,null,"Electric",null,"Total","#",0]
[null,null,null,null,"Residential buildings","#",0]
[null,null,null,null,"Public buildings","#",0]
[null,null,null,null,"Private buildings","#",0]
[null,null,"Thermal",null,"Total","#",0]
[null,null,null,null,"Residential buildings","#",0]
[null,null,null,null,"Public buildings","#",0]
[null,null,null,null,"Private buildings","#",0]
["# of buildings connected to a district thermal energy system",null,null,null,"Total","#",0]
[null,null,null,null,"Residential buildings","#",0]
[null,null,null,null,"Public buildings","#",0]
[null,null,null,null,"Private buildings","#",0]
["Use of secondary heat",null,null,null,null,"kWh"]
["Peak Load Consumption",null,"Total",null,null,"kW"]
[null,null,"Electric",null,null,"kW"]
[null,null,"Thermal DH",null,null,"kW"]
["Peak Load Production",null,"Total",null,null,"kW"]
[null,null,"Electric",null,null,"kW"]
[null,null,"Thermal DH",null,null,"kW"]
["Modal split",null,"Total",null,null,"%",100.00000000000003]
[null,null,"Bike/Walk",null,null,"%",17.371805759283564]
[null,null,"Fossil free Car",null,null,"%",4.2375448930749631]
[null,null,"Fossil fuel Car",null,null,"%",52.042776268046019]
[null,null,"Fossil free Public transport",null,null,"%",15.808723847757275]
[null,null,"Fossil fuel Public transport",null,null,"%",10.539149231838186]
["# filling stations with RES fuel for public access",null,"Total",null,null,"#"]
["CO2 emissions",null,"Total",null,null,"tonnes",738.94114777676657]
[null,null,"Stationary Energy","Total","Total","tonnes",598.73943446181534]
[null,null,null,null,"Residential buildings","tonnes",490.32525520580646]
[null,null,null,null,"Public buildings","tonnes",0]
[null,null,null,null,"Private buildings","tonnes",98.734005156163022]
[null,null,null,null,"Infrastructure","tonnes",9.6801740998458889]
[null,null,null,null,"Local Energy Plant","tonnes",0]
[null,null,null,"Electricity","Total","tonnes",598.73943446181534]
[null,null,null,null,"Residential buildings","tonnes",490.32525520580646]
[null,null,null,null,"Public buildings","tonnes",0]
[null,null,null,null,"Private buildings","tonnes",98.734005156163022]
[null,null,null,null,"Infrastructure","tonnes",9.6801740998458889]
[null,null,null,null,"Local Energy Plant","tonnes",0]
[null,null,null,"Biofuel","Total","tonnes",0]
[null,null,null,null,"Residential buildings","tonnes",0]
[null,null,null,null,"Public buildings","tonnes",0]
[null,null,null,null,"Private buildings","tonnes",0]
[null,null,null,null,"Infrastructure","tonnes",0]
[null,null,null,"Fossile fuel","Total","tonnes",0]
[null,null,null,null,"Residential buildings","tonnes",0]
[null,null,null,null,"Public buildings","tonnes",0]
[null,null,null,null,"Private buildings","tonnes",0]
[null,null,null,null,"Infrastructure","tonnes",0]
[null,null,null,"District heating","Total","tonnes",0]
[null,null,null,null,"Residential buildings","tonnes",0]
[null,null,null,null,"Public buildings","tonnes",0]
[null,null,null,null,"Private buildings","tonnes",0]
[null,null,null,null,"Infrastructure","tonnes",0]
[null,null,null,null,"Local Energy Plant","tonnes",0]
[null,null,"Mobility",null,"Total","tonnes",140.20171331495121]
[null,null,null,null,"Private cars","tonnes",89.693402821468553]
[null,null,null,null,"Public transport","tonnes",21.708815038937207]
[null,null,null,null,"Goods transport","tonnes",28.799495454545454]
[null,null,"Materials",null,"Total","tonnes",0]
[null,null,null,null,"Residential buildings","tonnes",0]
[null,null,null,null,"Public buildings","tonnes",0]
[null,null,null,null,"Private buildings","tonnes",0]
["# fossil free construction sites",null,"Total",null,"Total","#"]
[null,null,null,null,"Residential buildings","#"]
[null,null,null,null,"Public buildings","#"]
[null,null,null,null,"Private buildings","#"]
[null,null,"Construction Machines and Transportation",null,"Total","#"]
[null,null,null,null,"Residential buildings","#"]
[null,null,null,null,"Public buildings","#"]
[null,null,null,null,"Private buildings","#"]
[null,null,"Energy production",null,"Total","#"]
[null,null,null,null,"Residential buildings","#"]
[null,null,null,null,"Public buildings","#"]
[null,null,null,null,"Private buildings","#"]
["# of registered oil tanks",null,null,null,"Total","#"]
[null,null,null,null,"Residential buildings","#"]
[null,null,null,null,"Public buildings","#"]
[null,null,null,null,"Private buildings","#"]

{"sheet":"KPIs summary list","index":8,"n_rows":83,"n_cols":6,"rows_kept":83,"cut":false,"hidden":true,"merged":[[0,2,0,3]]}
["KPI","Goal s","Sub-categories",null,"Sectors","Unit"]
["Name","Name",1,2]
["CO2 emissions","CO2-reduction","Stationary Energy","Electricity","Public buildings","Tonnes CO2 eqv."]
[null,null,null,"Biofuel","Residential buildings"]
[null,null,null,"Fossile fuel","Private buildings"]
[null,null,null,"District heating","Infrastructure"]
[null,null,"Mobility",null,"Private cars"]
[null,null,null,null,"Taxi"]
[null,null,null,null,"Public transport"]
[null,null,null,null,"Goods transport"]
[null,null,null,null,"Freight transportation"]
[null,null,null,null,"Construction machines"]
[null,null,"Materials",null,"Public buildings"]
[null,null,null,null,"Residential buildings"]
[null,null,null,null,"Private buildings"]
["Energy Use","Increased energy efficiency","Electric","Buildings","Public buildings","MWh"]
[null,null,null,null,"Residential buildings"]
[null,null,null,null,"Private buildings"]
[null,null,null,"Infrastructure","Outdoor lighting"]
[null,null,null,null,"Transport"]
[null,null,null,null,"Other"]
[null,null,"Thermal","Solar","Public buildings"]
[null,null,null,"Biofuel","Residential buildings"]
[null,null,null,"Oil","Private buildings"]
[null,null,null,"Gas","Infrastructure"]
[null,null,null,"District heating"]
["District Heating share of renewables","Increased use of renewable energy","Electricity",null,null,"%"]
[null,null,"Heat pump"]
[null,null,"Solar"]
[null,null,"Biofuel"]
[null,null,"Waste"]
[null,null,"Oil"]
[null,null,"Gas"]
["Energy Certificate","Increased energy efficiency","Certificate A",null,"Public buildings","%"]
[null,null,"Certificate B",null,"Residential buildings"]
[null,null,"Certificate C",null,"Private buildings"]
[null,null,"Certificate D"]
[null,null,"Certificate E"]
[null,null,"Certificate F"]
[null,null,"Certificate G"]
[null,null,"Not registered"]
["Use of energy related incentive","Increased energy efficiency","Futurebuildt",null,"Public buildings","#"]
[null,null,"Enova",null,"Residential buildings"]
[null,null,"Local",null,"Private buildings"]
["Buildings benchmarked and measuring energy performance","Increased energy efficiency",null,null,"Public buildings","%"]
[null,null,null,null,"Residential buildings"]
[null,null,null,null,"Private buildings"]
["# fossile free construction sites","CO2-reduction","Construction Machines",null,"Public buildings","#"]
[null,"Increased use of renewable energy","Energy production",null,"Residential buildings"]
[null,null,null,null,"Private buildings"]
["Modal Split","Green mobility (reduced CO2 emissions and better air quality)","Fossil free Car",null,null,"%"]
[null,null,"Fossil fuel Car"]
[null,null,"Fossil free Public transport"]
[null,null,"Fossil fuel Public transport"]
[null,null,"Bike"]
[null,null,"Walk"]
["# filling stations with RES fuel / area/innh.","Green mobility (reduced CO2 emissions and better air quality)","Electric",null,null,"#"]
[null,null,"Hydrogen"]
[null,null,"Biofuel"]
["% fossil free cars of new car registerred","Green mobility (reduced CO2 emissions and better air quality)","Electric",null,null,"%"]
[null,null,"Hydrogen"]
["% of berths with power connection","Green mobility (reduced CO2 emissions and better air quality)"]
["RES installed capacity","Increased use of local energy sources","Electric","Solar",null,"kW"]
[null,"Increased use of renewable energy","Thermal","CHP Waste"]
[null,null,null,"CHP Biomass"]
["RES generated energy","Increased use of local energy sources","Electric","Solar",null,"MWh"]
[null,"Increased use of renewable energy","Thermal","CHP Waste"]
[null,null,null,"CHP Biomass"]
["Buildings with installed RES","Increased use of local energy sources","Electric","Solar",null,"%"]
[null,"Increased use of renewable energy","Thermal"]
["Use of secondary heat","Increased use of local energy sources",null,null,null,"MWh"]
["Buildings connected to a district thermal energy ","Increased use of local energy sources",null,null,null,"%"]
[null,"Increased use of renewable energy"]
["Identification of available resources of renewable energy","Increased use of local energy sources",null,null,null,"MWh"]
[null,"Increased use of renewable energy"]
["Number of registered oil tanks","Increased use of renewable energy",null,null,null,"#"]
[null,"CO2-reduction"]
["Peak Load Consumption",null,"Electric",null,null,"kW"]
[null,null,"Thermal"]
["Peak Load Production","Increased use of local energy sources","Electric",null,null,"kW"]
[null,null,"Thermal"]
["Energy Storage","Increased use of local energy sources","Electric",null,null,"MWh"]
[null,"Increased use of renewable energy","Thermal"]